(kicad_pcb (version 20171130) (host pcbnew 5.1.10)

  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 0)
    (zones 0)
    (modules 17)
    (nets 1)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "sweep2gerber"))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA241)
    (at 40 62.992)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604BAF06)
    (fp_text reference SW15 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA17E)
    (at 40 45.974)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A6D52)
    (fp_text reference SW9 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA157)
    (at 22 58)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A6C6C)
    (fp_text reference SW8 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA0BB)
    (at 40 29)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /6049E7C0)
    (fp_text reference SW3 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA094)
    (at 22 41)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /6049E323)
    (fp_text reference SW2 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA21A)
    (at 22 75)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604BAD64)
    (fp_text reference SW14 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA304)
    (at 85.97 81.7 165)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A14CA)
    (fp_text reference SW21 (at 4.98 -5.69 345) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 345) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 345) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255 165) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA2DD)
    (at 104.53 89.7 150)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A14C0)
    (fp_text reference SW20 (at 4.98 -5.690001 330) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.170001 330) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 330) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255 150) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA2B6)
    (at 93.98 64.008)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604BAF24)
    (fp_text reference SW18 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA28F)
    (at 76 61.468)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604BAF1A)
    (fp_text reference SW17 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA268)
    (at 58 56.134)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604BAF10)
    (fp_text reference SW16 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA1F3)
    (at 93.98 46.99)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A6D70)
    (fp_text reference SW12 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA1CC)
    (at 76 44.45)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A6D66)
    (fp_text reference SW11 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA1A5)
    (at 58 39.116)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /604A6D5C)
    (fp_text reference SW10 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA130)
    (at 94 30)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /6049F698)
    (fp_text reference SW6 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA109)
    (at 76 27.5)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /6049F636)
    (fp_text reference SW5 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (module Kailh:SW_PG1350_cut (layer F.Cu) (tedit 5F05DFF4) (tstamp 608AA0E2)
    (at 58 22)
    (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
    (tags kailh,choc)
    (path /6049EB70)
    (fp_text reference SW4 (at 4.98 -5.69 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Push (at -0.07 8.17 180) (layer Dwgs.User) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %V (at 0 8.255) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -7 -7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -7 7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  )

  (gr_line (start 118.618 81.28) (end 105.918 81.28) (layer Edge.Cuts) (width 0.05) (tstamp 60FE80A0))
  (gr_line (start 105.918 81.28) (end 105.918 74.422) (layer Edge.Cuts) (width 0.05) (tstamp 60FE8097))
  (gr_line (start 103.124 74.422) (end 105.918 74.422) (layer Edge.Cuts) (width 0.05) (tstamp 60FE8093))
  (gr_line (start 103.124 72.39) (end 103.124 74.422) (layer Edge.Cuts) (width 0.05) (tstamp 60FE8090))
  (gr_line (start 103.124 72.39) (end 102.108 72.39) (layer Edge.Cuts) (width 0.05) (tstamp 60FE8062))
  (gr_line (start 64.211777 13.120679) (end 60.010389 13.126139) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEBF))
  (gr_line (start 118.618 81.28) (end 108.59 99.069265) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEBD))
  (gr_arc (start 60.010389 81.856139) (end 60.010389 13.126139) (angle -40.87028694) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEBC))
  (gr_line (start 102.108 72.39) (end 102.142045 22.057419) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEBA))
  (gr_arc (start 15.628253 81.018608) (end 13.650254 81.165024) (angle -87.49275882) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB8))
  (gr_arc (start 15.109962 406.957453) (end 84.329134 90.481946) (angle -12.23515303) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB7))
  (gr_arc (start 106.928 98.018) (end 105.858 99.668) (angle -90.64821197) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB6))
  (gr_arc (start 52.264442 156.650303) (end 101.70729 21.376889) (angle -15.31921041) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB5))
  (gr_arc (start 17.482 33.128) (end 15.037 29.883) (angle -35.36225308) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB3))
  (gr_arc (start 61.542 173.708) (end 105.858 99.668) (angle -15.59005573) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB2))
  (gr_arc (start 101.392045 22.057419) (end 102.142045 22.057419) (angle -65.14479855) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB1))
  (gr_line (start 13.610055 31.896702) (end 13.650254 81.165024) (layer Edge.Cuts) (width 0.05) (tstamp 608AAEB0))

)
