(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "MJ-4PP-9" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MJ-4PP-9" (at 0 -3.81 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 6.985 4.445 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 6.985 4.445 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio jack receptable stereo headphones TRRS connector" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "4-pin (audio) jack receptable (stereo + 4th pin/TRRS connector), compatible with PJ320A" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MJ-4PP-9_0_1"
      (rectangle (start -1.905 -1.905) (end -3.175 1.27)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -2.54 1.27)
          (xy -2.54 1.905)
          (xy 3.175 1.905)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 -1.905)
          (xy -0.635 -1.27)
          (xy 0 -1.905)
          (xy 3.175 -1.905)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -0.635)
          (xy 0.635 0)
          (xy 1.27 -0.635)
          (xy 3.175 -0.635)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.27 0.635)
          (xy 1.905 1.27)
          (xy 2.54 0.635)
          (xy 3.175 0.635)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (rectangle (start 3.175 2.54) (end -3.81 -2.54)
        (stroke (width 0.3048) (type solid))
        (fill (type none))
      )
    )
    (symbol "MJ-4PP-9_1_1"
      (pin input line (at 5.08 1.905 180) (length 2.0066)
        (name "~" (effects (font (size 0.508 0.508))))
        (number "A" (effects (font (size 0.7112 0.7112))))
      )
      (pin input line (at 5.08 -1.905 180) (length 2.0066)
        (name "~" (effects (font (size 0.508 0.508))))
        (number "B" (effects (font (size 0.7112 0.7112))))
      )
      (pin input line (at 5.08 -0.635 180) (length 2.0066)
        (name "~" (effects (font (size 0.508 0.508))))
        (number "C" (effects (font (size 0.7112 0.7112))))
      )
      (pin input line (at 5.08 0.635 180) (length 2.0066)
        (name "~" (effects (font (size 0.508 0.508))))
        (number "D" (effects (font (size 0.7112 0.7112))))
      )
    )
  )
  (symbol "OLED" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "OL" (at 0 2.54 0)
      (effects (font (size 1.2954 1.2954)))
    )
    (property "Value" "OLED" (at 0 -1.27 0)
      (effects (font (size 1.1938 1.1938)))
    )
    (property "Footprint" "" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "OLED_0_1"
      (rectangle (start -13.97 8.89) (end 15.24 -7.62)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "OLED_1_1"
      (pin bidirectional line (at -19.05 6.35 0) (length 5.08)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 2.54 0) (length 5.08)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -19.05 -1.27 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -19.05 -5.08 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ProMicro" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 19.05 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "ProMicro" (at 0 -19.05 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (at 2.54 -26.67 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (at 2.54 -26.67 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "ProMicro_0_1"
      (rectangle (start -12.7 16.51) (end 12.7 -16.51)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "ProMicro_1_1"
      (pin bidirectional line (at -17.78 13.97 0) (length 5.08)
        (name "TX0/D3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -8.89 0) (length 5.08)
        (name "7/E6" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -11.43 0) (length 5.08)
        (name "8/B4" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -13.97 0) (length 5.08)
        (name "9/B5" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -13.97 180) (length 5.08)
        (name "B6/10" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -11.43 180) (length 5.08)
        (name "B2/16" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 5.08)
        (name "B3/14" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -6.35 180) (length 5.08)
        (name "B1/15" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -3.81 180) (length 5.08)
        (name "F7/A0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -1.27 180) (length 5.08)
        (name "F6/A1" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 5.08)
        (name "F5/A2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 11.43 0) (length 5.08)
        (name "RX1/D2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 5.08)
        (name "F4/A3" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 6.35 180) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 8.89 180) (length 5.08)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 11.43 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 17.78 13.97 180) (length 5.08)
        (name "RAW" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 8.89 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -17.78 6.35 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 3.81 0) (length 5.08)
        (name "2/D1/SDA" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 1.27 0) (length 5.08)
        (name "3/D0/SCL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -1.27 0) (length 5.08)
        (name "4/D4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -3.81 0) (length 5.08)
        (name "5/C6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -6.35 0) (length 5.08)
        (name "6/D7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ProMicro_r" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 1.27 22.86 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "ProMicro_r" (at 1.27 -15.24 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (at 3.81 -26.67 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (at 3.81 -26.67 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "ProMicro_r_0_1"
      (rectangle (start 13.97 20.32) (end -11.43 -12.7)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "ProMicro_r_1_1"
      (pin bidirectional line (at 19.05 17.78 180) (length 5.08)
        (name "D3/TX0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 -5.08 180) (length 5.08)
        (name "E6/7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 -7.62 180) (length 5.08)
        (name "B4/8" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 -10.16 180) (length 5.08)
        (name "B5/9" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -10.16 0) (length 5.08)
        (name "10/B6" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -7.62 0) (length 5.08)
        (name "16/B2" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -5.08 0) (length 5.08)
        (name "14/B3" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 -2.54 0) (length 5.08)
        (name "15/B1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 0 0) (length 5.08)
        (name "A0/F7" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 2.54 0) (length 5.08)
        (name "A1/F6" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 5.08 0) (length 5.08)
        (name "A2/F5" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 15.24 180) (length 5.08)
        (name "D2/RX1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -16.51 7.62 0) (length 5.08)
        (name "A3/F4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 10.16 0) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 12.7 0) (length 5.08)
        (name "RST" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -16.51 15.24 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -16.51 17.78 0) (length 5.08)
        (name "RAW" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 12.7 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.05 10.16 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 7.62 180) (length 5.08)
        (name "SDA/D1/2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 5.08 180) (length 5.08)
        (name "SCL/D0/3" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 2.54 180) (length 5.08)
        (name "D4/4" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 0 180) (length 5.08)
        (name "C6/5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 19.05 -2.54 180) (length 5.08)
        (name "D7/6" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SELIAL_LED_TEAP" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "L" (at 0 2.54 0)
      (effects (font (size 1.2954 1.2954)))
    )
    (property "Value" "SELIAL_LED_TEAP" (at 0 -1.27 0)
      (effects (font (size 1.1938 1.1938)))
    )
    (property "Footprint" "" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (at 0 2.54 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "SELIAL_LED_TEAP_0_1"
      (rectangle (start -13.97 6.35) (end 15.24 -6.35)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "SELIAL_LED_TEAP_1_1"
      (pin power_in line (at 20.32 3.81 180) (length 5.08)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 0 180) (length 5.08)
        (name "Din" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 -3.81 180) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -19.05 3.81 0) (length 5.08)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -19.05 0 0) (length 5.08)
        (name "DO" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -19.05 -3.81 0) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SK6812MINI" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "L" (at 0 0 0)
      (effects (font (size 1.2954 1.2954)))
    )
    (property "Value" "SK6812MINI" (at 0 -1.27 0)
      (effects (font (size 0.4064 0.4064)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "SK6812MINI_0_1"
      (rectangle (start -3.81 3.81) (end 3.81 -3.81)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
    )
    (symbol "SK6812MINI_1_1"
      (pin output line (at -5.08 2.54 0) (length 1.1938)
        (name "DOUT" (effects (font (size 0.7112 0.7112))))
        (number "1" (effects (font (size 0.7112 0.7112))))
      )
      (pin power_in line (at -5.08 -2.54 0) (length 1.1938)
        (name "VSS" (effects (font (size 0.7112 0.7112))))
        (number "2" (effects (font (size 0.7112 0.7112))))
      )
      (pin input line (at 5.08 -2.54 180) (length 1.1938)
        (name "DIN" (effects (font (size 0.7112 0.7112))))
        (number "3" (effects (font (size 0.7112 0.7112))))
      )
      (pin power_in line (at 5.08 2.54 180) (length 1.1938)
        (name "VDD" (effects (font (size 0.7112 0.7112))))
        (number "4" (effects (font (size 0.7112 0.7112))))
      )
    )
  )
  (symbol "SW_PUSH" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (at 3.81 2.794 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SW_PUSH" (at 0 -2.032 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "SW_PUSH_0_1"
      (rectangle (start -4.318 1.27) (end 4.318 1.524)
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.016 1.524)
          (xy -0.762 2.286)
          (xy 0.762 2.286)
          (xy 1.016 1.524)
        )
        (stroke (width 0) (type solid))
        (fill (type none))
      )
      (pin passive inverted (at -7.62 0 0) (length 5.08)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive inverted (at 7.62 0 180) (length 5.08)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "YS-SK6812MINI-E" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "LED" (at 2.54 -7.62 0)
      (effects (font (size 0.7366 0.7366)))
    )
    (property "Value" "YS-SK6812MINI-E" (at 6.35 -6.35 0)
      (effects (font (size 0.7366 0.7366)))
    )
    (property "Footprint" "" (at 2.54 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 2.54 -6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "YS-SK6812MINI-E_0_1"
      (rectangle (start -5.08 5.08) (end 5.08 -5.08)
        (stroke (width 0.254) (type solid))
        (fill (type background))
      )
    )
    (symbol "YS-SK6812MINI-E_1_1"
      (pin power_in line (at 0 7.62 270) (length 2.54)
        (name "VDD" (effects (font (size 0.9906 0.9906))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "DOUT" (effects (font (size 0.9906 0.9906))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -7.62 90) (length 2.54)
        (name "VSS" (effects (font (size 0.9906 0.9906))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "DIN" (effects (font (size 0.9906 0.9906))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
