EESchema-DOCLIB  Version 2.0
#
$CMP 4P2C
D RJ connector, 4P2C (4 positions 2 connected)
K 4P2C RJ female connector
F ~
$ENDCMP
#
$CMP 4P2C_Shielded
D RJ connector, 4P2C (4 positions 2 connected), Shielded
K 4P2C RJ female connector
F ~
$ENDCMP
#
$CMP 4P4C
D RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP 4P4C_Shielded
D RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22, Shielded
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP 6P2C
D RJ connector, 6P2C (6 positions 2 connected), RJ11
K 6P2C RJ female connector
F ~
$ENDCMP
#
$CMP 6P2C_Shielded
D RJ connector, 6P2C (6 positions 2 connected), RJ11, Shielded
K 6P2C RJ female connector
F ~
$ENDCMP
#
$CMP 6P4C
D RJ connector, 6P4C (6 positions 4 connected), RJ13/RJ14
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP 6P4C_Shielded
D RJ connector, 6P4C (6 positions 4 connected), RJ13/RJ14, Shielded
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP 6P6C
D RJ connector, 6P6C (6 positions 6 connected), RJ12/RJ18/RJ25
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP 6P6C_Shielded
D RJ connector, 6P6C (6 positions 6 connected), RJ12/RJ18/RJ25, Shielded
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP 8P4C
D RJ connector, 8P4C (8 positions 4 connected), RJ38/RJ48
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP 8P4C_Shielded
D RJ connector, 8P4C (8 positions 4 connected), RJ38/RJ48, Shielded
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP 8P8C
D RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP 8P8C_LED
D RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45
K 8P8C RJ female connector led
F ~
$ENDCMP
#
$CMP 8P8C_LED_Shielded
D RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded
K 8P8C RJ female connector led
F ~
$ENDCMP
#
$CMP 8P8C_LED_Shielded_x2
D RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded, two ports
K 8P8C RJ female connector led dual
F ~
$ENDCMP
#
$CMP 8P8C_Shielded
D RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61, Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP ATX-20
D ATX Power supply 20pins
K ATX PSU
F https://web.aub.edu.lb/pub/docs/atx_201.pdf#page=20
$ENDCMP
#
$CMP ATX-24
D ATX Power supply 24pins
K ATX PSU
F https://www.intel.com/content/dam/www/public/us/en/documents/guides/power-supply-design-guide-june.pdf#page=33
$ENDCMP
#
$CMP AVR-ISP-10
D Atmel 10-pin ISP connector
K AVR ISP Connector
F  ~
$ENDCMP
#
$CMP AVR-ISP-6
D Atmel 6-pin ISP connector
K AVR ISP Connector
F  ~
$ENDCMP
#
$CMP AVR-JTAG-10
D Atmel 10-pin JTAG connector
K AVR JTAG Connector
F  ~
$ENDCMP
#
$CMP AVR-PDI-6
D Atmel 6-pin PDI connector
K AVR PDI Connector
F  ~
$ENDCMP
#
$CMP AVR-TPI-6
D Atmel 6-pin TPI connector
K AVR TPI Connector
F  ~
$ENDCMP
#
$CMP AVR-UPDI-6
D Atmel 6-pin UPDI connector
K AVR UPDI Connector
F https://www.microchip.com/webdoc/GUID-9D10622A-5C16-4405-B092-1BDD437B4976/index.html?GUID-9B349315-2842-4189-B88C-49F4E1055D7F
$ENDCMP
#
$CMP AudioJack2
D Audio Jack, 2 Poles (Mono / TS)
K audio jack receptacle mono phone headphone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Dual_Ground_Switch
D Audio Jack, Dual, 2 Poles (Mono / TS), Grounded Sleeve, Switched Pole (Normalling)
K audio jack dual receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Dual_Switch
D Audio Jack, Dual, 2 Poles (Mono / TS), Switched Pole (Normalling)
K audio jack dual receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Ground
D Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve
K audio jack receptacle mono phone headphone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Ground_Switch
D Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve, Switched Pole (Normalling)
K audio jack receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Ground_SwitchT
D Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve, Switched T Pole (Normalling)
K audio jack receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_Switch
D Audio Jack, 2 Poles (Mono / TS), Switched Pole (Normalling)
K audio jack receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack2_SwitchT
D Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)
K audio jack receptacle mono headphones phone TS connector
F ~
$ENDCMP
#
$CMP AudioJack3
D Audio Jack, 3 Poles (Stereo / TRS)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Dual_Ground_Switch
D Audio Jack, Dual, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched Poles (Normalling)
K audio jack dual receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Dual_Switch
D Audio Jack, Dual, 3 Poles (Stereo / TRS), Switched Poles (Normalling)
K audio jack dual receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Ground
D Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Ground_Switch
D Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched Poles (Normalling)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Ground_SwitchTR
D Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched TR Poles (Normalling)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack3_Switch
D Audio Jack, 3 Poles (Stereo / TRS), Switched Poles (Normalling)
K audio jack receptacle stereo headphones connector
F ~
$ENDCMP
#
$CMP AudioJack3_SwitchTR
D Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack4
D Audio Jack, 4 Poles (TRRS)
K audio jack receptacle stereo headphones TRRS connector
F ~
$ENDCMP
#
$CMP AudioJack4_Ground
D Audio Jack, 4 Poles (TRRS), Grounded Sleeve
K audio jack receptacle stereo headphones TRRS connector
F ~
$ENDCMP
#
$CMP AudioJack4_Ground_SwitchTR1
D Audio Jack, 4 Poles (Stereo / TRRS), Grounded Sleeve, Switched TR1 Poles (Normalling)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack4_SwitchTR1
D Audio Jack, 4 Poles (Stereo / TRRS), Switched TR1 Poles (Normalling)
K audio jack receptacle stereo headphones phones TRS connector
F ~
$ENDCMP
#
$CMP AudioJack4dpb
D Audio Jack, 4 Poles (TRRS)
K audio jack receptacle stereo headphones TRRS connector
F ~
$ENDCMP
#
$CMP AudioJack5
D Audio Jack, 5 Poles (TRRRS)
K audio jack receptacle stereo headphones TRRRS connector
F ~
$ENDCMP
#
$CMP AudioJack5_Ground
D Audio Jack, 5 Poles (TRRRS), Grounded Sleeve
K audio jack receptacle stereo headphones TRRRS connector
F ~
$ENDCMP
#
$CMP AudioPlug2
D Audio Jack, 2 Poles (Mono / TS)
K audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm 6.35mm
F ~
$ENDCMP
#
$CMP AudioPlug3
D Audio Jack, 3 Poles (Stereo / TRS)
K audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm 6.35mm
F ~
$ENDCMP
#
$CMP AudioPlug4
D Audio Jack, 4 Poles (Stereo / TRRS)
K audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm
F ~
$ENDCMP
#
$CMP Barrel_Jack
D DC Barrel Jack
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Barrel_Jack_MountingPin
D DC Barrel Jack with a mounting pin
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Barrel_Jack_Switch
D DC Barrel Jack with an internal switch
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Barrel_Jack_Switch_MountingPin
D DC Barrel Jack with an internal switch and a mounting pin
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Barrel_Jack_Switch_Pin3Ring
D DC Barrel Jack with an internal switch
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP Bus_ISA_16bit
D 16-bit ISA-AT bus connector
K ISA
F https://en.wikipedia.org/wiki/Industry_Standard_Architecture
$ENDCMP
#
$CMP Bus_ISA_8bit
D 8-bit ISA-PC bus connector
K ISA
F https://en.wikipedia.org/wiki/Industry_Standard_Architecture
$ENDCMP
#
$CMP Bus_PCI_32bit_5V
D PCI bus connector for 5V cards
K PCI 5V
F http://pinouts.ru/Slots/PCI_pinout.shtml
$ENDCMP
#
$CMP Bus_PCI_32bit_Universal
D PCI bus connector for universal 5V/3.3V cards
K PCI 5V 3.3V 3V3
F http://pinouts.ru/Slots/PCI_pinout.shtml
$ENDCMP
#
$CMP Bus_PCI_Express_Mini
D Mini-PCI Express bus connector
K mini pcie
F ~
$ENDCMP
#
$CMP C64AB
D Connector Europe 64 contacts ranges A,B
K connector DIN
F  ~
$ENDCMP
#
$CMP C64AC
D Connector Europe 64 contacts, ranges A,B,C
K connector DIN
F  ~
$ENDCMP
#
$CMP C96ABC
D Connector Europe, 96 contacts, ranges A,B,C
K connector
F  ~
$ENDCMP
#
$CMP CUI_PD-30
D 3 pin connector, PD-30
K connector 3-pin PD-30 power DIN
F http://www.cui.com/product/resource/pd-30.pdf
$ENDCMP
#
$CMP CoaxialSwitch_Testpoint
D Subminiature Coaxial Switch testpoint
K  Coaxial Switch RF testpoint
F ~
$ENDCMP
#
$CMP Conn_01x01_Female
D Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x01_Male
D Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02_Female
D Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02_Male
D Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03_Female
D Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03_Male
D Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04_Female
D Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04_Male
D Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x05_Female
D Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x05_Male
D Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x06_Female
D Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x06_Male
D Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x07_Female
D Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x07_Male
D Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x08_Female
D Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x08_Male
D Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x09_Female
D Generic connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x09_Male
D Generic connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x10_Female
D Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x10_Male
D Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x11_Female
D Generic connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x11_Male
D Generic connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x12_Female
D Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x12_Male
D Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x13_Female
D Generic connector, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x13_Male
D Generic connector, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x14_Female
D Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x14_Male
D Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x15_Female
D Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x15_Male
D Generic connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x16_Female
D Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x16_Male
D Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x17_Female
D Generic connector, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x17_Male
D Generic connector, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x18_Female
D Generic connector, single row, 01x18, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x18_Male
D Generic connector, single row, 01x18, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x19_Female
D Generic connector, single row, 01x19, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x19_Male
D Generic connector, single row, 01x19, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x20_Female
D Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x20_Male
D Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x21_Female
D Generic connector, single row, 01x21, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x21_Male
D Generic connector, single row, 01x21, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x22_Female
D Generic connector, single row, 01x22, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x22_Male
D Generic connector, single row, 01x22, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x23_Female
D Generic connector, single row, 01x23, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x23_Male
D Generic connector, single row, 01x23, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x24_Female
D Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x24_Male
D Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x25_Female
D Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x25_Male
D Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x26_Female
D Generic connector, single row, 01x26, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x26_Male
D Generic connector, single row, 01x26, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x27_Female
D Generic connector, single row, 01x27, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x27_Male
D Generic connector, single row, 01x27, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x28_Female
D Generic connector, single row, 01x28, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x28_Male
D Generic connector, single row, 01x28, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x29_Female
D Generic connector, single row, 01x29, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x29_Male
D Generic connector, single row, 01x29, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x30_Female
D Generic connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x30_Male
D Generic connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x31_Female
D Generic connector, single row, 01x31, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x31_Male
D Generic connector, single row, 01x31, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x32_Female
D Generic connector, single row, 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x32_Male
D Generic connector, single row, 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x33_Female
D Generic connector, single row, 01x33, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x33_Male
D Generic connector, single row, 01x33, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x34_Female
D Generic connector, single row, 01x34, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x34_Male
D Generic connector, single row, 01x34, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x35_Female
D Generic connector, single row, 01x35, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x35_Male
D Generic connector, single row, 01x35, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x36_Female
D Generic connector, single row, 01x36, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x36_Male
D Generic connector, single row, 01x36, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x37_Female
D Generic connector, single row, 01x37, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x37_Male
D Generic connector, single row, 01x37, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x38_Female
D Generic connector, single row, 01x38, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x38_Male
D Generic connector, single row, 01x38, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x39_Female
D Generic connector, single row, 01x39, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x39_Male
D Generic connector, single row, 01x39, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x40_Female
D Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x40_Male
D Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_15X4
D Connector Europe, 60 contacts, ranges A,B,C,D
K connector
F  ~
$ENDCMP
#
$CMP Conn_ARM_JTAG_SWD_10
D Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface
K Cortex Debug Connector ARM SWD JTAG
F http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf
$ENDCMP
#
$CMP Conn_ARM_JTAG_SWD_20
D Standard IDC20 Male Connector, ARM legacy JTAG and SWD interface
K IDC20 Male Connector ARM JTAG SWD
F http://infocenter.arm.com/help/topic/com.arm.doc.dui0499b/DUI0499B_system_design_reference.pdf
$ENDCMP
#
$CMP Conn_Coaxial
D coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
F  ~
$ENDCMP
#
$CMP Conn_Coaxial_Power
D coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
F ~
$ENDCMP
#
$CMP Conn_Coaxial_x2
D double coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
F  ~
$ENDCMP
#
$CMP Conn_Coaxial_x2_Isolated
D coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)
K BNC SMA SMB SMC coaxial connector CINCH RCA
F  ~
$ENDCMP
#
$CMP Conn_PIC_ICSP_ICD
D Microchip PIC In-Circuit Serial Programming/Debugging (ICSP/ICD) connector
K icsp icd pic microchip
F http://ww1.microchip.com/downloads/en/devicedoc/30277d.pdf
$ENDCMP
#
$CMP Conn_ST_STDC14
D ST Debug Connector, standard ARM Cortex-M SWD and JTAG interface plus UART
K ST STM32 Cortex Debug Connector ARM SWD JTAG
F https://www.st.com/content/ccc/resource/technical/document/user_manual/group1/99/49/91/b6/b2/3a/46/e5/DM00526767/files/DM00526767.pdf/jcr:content/translations/en.DM00526767.pdf
$ENDCMP
#
$CMP Conn_WallPlug
D 3-pin general wall plug, no Earth wire (110VAC, 220VAC)
K wall plug 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallPlug_Earth
D 3-pin general wall plug, with Earth wire (110VAC, 220VAC)
K wall plug 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallSocket
D 3-pin german wall socket, no Earth wire (110VAC, 220VAC)
K wall socket 110VAC 220VAC
F ~
$ENDCMP
#
$CMP Conn_WallSocket_Earth
D 3-pin german wall socket, with Earth wire (110VAC, 220VAC)
K wall socket 110VAC 220VAC
F ~
$ENDCMP
#
$CMP DB15_Female
D 15-pin female D-SUB connector (low-density/2 columns)
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB15_Female_HighDensity
D 15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector
K connector db15 VGA female D-SUB
F  ~
$ENDCMP
#
$CMP DB15_Female_HighDensity_MountingHoles
D 15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole
K connector db15 female D-SUB VGA
F  ~
$ENDCMP
#
$CMP DB15_Female_MountingHoles
D 15-pin female D-SUB connector (low-density/2 columns), Mounting Hole
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB15_Male
D 15-pin male D-SUB connector (low-density/2 columns)
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB15_Male_HighDensity
D 15-pin male D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector
K connector male VGA D-SUB
F  ~
$ENDCMP
#
$CMP DB15_Male_HighDensity_MountingHoles
D 15-pin male D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole
K connector male D-SUB VGA
F  ~
$ENDCMP
#
$CMP DB15_Male_MountingHoles
D 15-pin male D-SUB connector (low-density/2 columns), Mounting Hole
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB25_Female
D 25-pin female D-SUB connector
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB25_Female_MountingHoles
D 25-pin female D-SUB connector, Mounting Hole
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB25_Male
D 25-pin male D-SUB connector
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB25_Male_MountingHoles
D 25-pin male D-SUB connector, Mounting Hole
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB37_Female
D 37-pin female D-SUB connector
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB37_Female_MountingHoles
D 37-pin female D-SUB connector, Mounting Hole
K female D-SUB connector
F  ~
$ENDCMP
#
$CMP DB37_Male
D 37-pin male D-SUB connector
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB37_Male_MountingHoles
D 37-pin male D-SUB connector, Mounting Hole
K male D-SUB connector
F  ~
$ENDCMP
#
$CMP DB9_Female
D 9-pin female D-SUB connector
K connector female D-SUB
F  ~
$ENDCMP
#
$CMP DB9_Female_MountingHoles
D 9-pin female D-SUB connector, Mounting Hole
K connector female D-SUB
F  ~
$ENDCMP
#
$CMP DB9_Male
D 9-pin male D-SUB connector
K connector male D-SUB
F  ~
$ENDCMP
#
$CMP DB9_Male_MountingHoles
D 9-pin male D-SUB connector, Mounting Hole
K connector male D-SUB
F  ~
$ENDCMP
#
$CMP DIN-3
D 3-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-4
D 4-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-5
D 5-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-5_180degree
D 5-pin DIN connector (5-pin DIN-5 stereo)
K circular DIN connector stereo audio
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-6
D 6-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-7
D 7-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-7_CenterPin7
D 7-pin DIN connector with pin 7 in center
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP DIN-8
D 8-pin DIN connector
K circular DIN connector
F http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf
$ENDCMP
#
$CMP ExpressCard
D ExpressCard connector
K expresscard pci express
F https://web.archive.org/web/20180809060653/http://www.usb.org/developers/expresscard/EC_specifications/ExpressCard_2_0_FINAL.pdf
$ENDCMP
#
$CMP HDMI_A
D HDMI type A connector
K hdmi conn
F https://en.wikipedia.org/wiki/HDMI
$ENDCMP
#
$CMP HDMI_A_1.4
D HDMI 1.4+ type A connector
K hdmi conn
F https://en.wikipedia.org/wiki/HDMI
$ENDCMP
#
$CMP HDMI_B
D HDMI type B connector
K hdmi conn
F http://pinouts.ru/Video/hdmi_pinout.shtml
$ENDCMP
#
$CMP HDMI_C_1.3
D HDMI 1.3+ type C connector
K hdmi conn
F http://pinoutguide.com/PortableDevices/mini_hdmi_pinout.shtml
$ENDCMP
#
$CMP HDMI_C_1.4
D HDMI 1.4+ type C connector
K hdmi conn
F http://pinoutguide.com/PortableDevices/mini_hdmi_pinout.shtml
$ENDCMP
#
$CMP HDMI_D_1.4
D HDMI 1.4+ type D connector
K hdmi conn
F http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml
$ENDCMP
#
$CMP HDMI_E
D HDMI type E connector
K hdmi conn
F https://www.hdmi.org/manufacturer/specification.aspx
$ENDCMP
#
$CMP IEEE1394a
D FireWire/IEEE1394a 6-pin connector
K connector IEEE1394a FireWire
F ~
$ENDCMP
#
$CMP JAE_SIM_Card_SF72S006
D Nano-SIM Card (4FF) connector with Detect Switch
K SIM card UICC 4FF
F https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809
$ENDCMP
#
$CMP JK0654219
D  1 Port RJ45 Magjack Connector Through Hole 10/100/1000 Base-T, AutoMDIX
K 8P8C RJ female connector
F https://media.digikey.com/pdf/Data%20Sheets/Pulse%20PDFs/JK%20Series.pdf
$ENDCMP
#
$CMP Jack-DC
D DC Barrel Jack
K DC power barrel jack connector
F ~
$ENDCMP
#
$CMP LEMO2
D 2-pin LEMO connector
K LEMO connector
F  ~
$ENDCMP
#
$CMP LEMO4
D 4-pin LEMO connector
K LEMO connector
F  ~
$ENDCMP
#
$CMP LEMO5
D 5-pin LEMO connector
K LEMO connector
F  ~
$ENDCMP
#
$CMP LEMO6
D 6-pin LEMO connector
K LEMO connector
F  ~
$ENDCMP
#
$CMP MXM3.0
D MXM3.0 connector
K MXM connector
F ~
$ENDCMP
#
$CMP Micro_SD_Card
D Micro SD Card Socket
K connector SD microsd
F http://katalog.we-online.de/em/datasheet/693072010801.pdf
$ENDCMP
#
$CMP Micro_SD_Card_Det
D Micro SD Card Socket with card detection pins
K connector SD microsd
F https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1
$ENDCMP
#
$CMP Micro_SD_Card_Det_Hirose_DM3AT
D Micro SD Card Socket with card detection pins
K connector SD microsd
F https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1
$ENDCMP
#
$CMP Microsemi_FlashPro-JTAG-10
D ACTEL FLASH PRO 3/4, JTAG, IDC10 Male Connector
K JTAG IDC10 Male Connector
F https://www.microsemi.com/document-portal/doc_view/129973-lpf-ac386-an
$ENDCMP
#
$CMP Mini-DIN-3
D 3-pin Mini-DIN connector
K Mini-DIN
F http://www.assmann-wsw.com/fileadmin/catalogue/10_MiniDIN_rev4-0.pdf
$ENDCMP
#
$CMP Mini-DIN-4
D 4-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-5
D 5-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-6
D 6-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-7
D 7-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Mini-DIN-8
D 8-pin Mini-DIN connector
K Mini-DIN
F http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf
$ENDCMP
#
$CMP Pulse_JXD6-0001NL
D LAN Transformer Jack, RJ45, 10/100 BaseT
K lan jack transformer
F https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/JXD6-0001NL/doc_part/JXD6-0001NL.pdf
$ENDCMP
#
$CMP RJ10
D RJ connector, 4P4C (4 positions 4 connected)
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ10_Shielded
D RJ connector, 4P4C (4 positions 4 connected), Shielded
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ11
D RJ connector, 6P2C (6 positions 2 connected)
K 6P2C RJ female connector
F ~
$ENDCMP
#
$CMP RJ11_Shielded
D RJ connector, 6P2C (6 positions 2 connected), Shielded
K 6P2C RJ female connector
F ~
$ENDCMP
#
$CMP RJ12
D RJ connector, 6P6C (6 positions 6 connected)
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ12_Shielded
D RJ connector, 6P6C (6 positions 6 connected), Shielded
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ13
D RJ connector, 6P4C (6 positions 4 connected)
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ13_Shielded
D RJ connector, 6P4C (6 positions 4 connected), Shielded
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ14
D RJ connector, 6P4C (6 positions 4 connected)
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ14_Shielded
D RJ connector, 6P4C (6 positions 4 connected), Shielded
K 6P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ18
D RJ connector, 6P6C (6 positions 6 connected)
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ18_Shielded
D RJ connector, 6P6C (6 positions 6 connected), Shielded
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ22
D RJ connector, 4P4C (4 positions 4 connected)
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ22_Shielded
D RJ connector, 4P4C (4 positions 4 connected), Shielded
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ25
D RJ connector, 6P6C (6 positions 6 connected)
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ25_Shielded
D RJ connector, 6P6C (6 positions 6 connected), Shielded
K 6P6C RJ female connector
F ~
$ENDCMP
#
$CMP RJ31
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ31_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ32
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ32_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ33
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ33_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ34
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ34_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ35
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ35_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ38
D RJ connector, 8P4C (8 positions 4 connected)
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ38_Shielded
D RJ connector, 8P4C (8 positions 4 connected), Shielded
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ41
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ41_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ45
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ45_Abracon_ARJP11A-MASA-B-A-EMU2
D RJ45 PoE 10/100 Base-TX Jack with Magnetic Module
K single port ethernet transformer poe center-tap
F https://abracon.com/Magnetics/lan/ARJP11A.PDF
$ENDCMP
#
$CMP RJ45_Amphenol_RJMG1BD3B8K1ANR
D 1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX
K RJ45 Magjack
F https://www.amphenolcanada.com/ProductSearch/Drawings/AC/RJMG1BD3B8K1ANR.PDF
$ENDCMP
#
$CMP RJ45_LED
D RJ connector, 8P8C (8 positions 8 connected), two LEDs
K 8P8C RJ female connector led
F ~
$ENDCMP
#
$CMP RJ45_LED_Shielded
D RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded
K 8P8C RJ female connector led
F ~
$ENDCMP
#
$CMP RJ45_LED_Shielded_x2
D RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded, two ports
K 8P8C RJ female connector led
F ~
$ENDCMP
#
$CMP RJ45_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ48
D RJ connector, 8P4C (8 positions 4 connected)
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ48_Shielded
D RJ connector, 8P4C (8 positions 4 connected), Shielded
K 8P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ49
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ49_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ61
D RJ connector, 8P8C (8 positions 8 connected)
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ61_Shielded
D RJ connector, 8P8C (8 positions 8 connected), Shielded
K 8P8C RJ female connector
F ~
$ENDCMP
#
$CMP RJ9
D RJ connector, 4P4C (4 positions 4 connected)
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP RJ9_Shielded
D RJ connector, 4P4C (4 positions 4 connected), Shielded
K 4P4C RJ female connector
F ~
$ENDCMP
#
$CMP Raspberry_Pi_2_3
D expansion header for Raspberry Pi 2 & 3
K raspberrypi gpio
F https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf
$ENDCMP
#
$CMP SCART-F
D Prise Peritel
K connector
F  ~
$ENDCMP
#
$CMP SD_Card
D SD Card Reader
K connector SD
F http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf
$ENDCMP
#
$CMP SIM_Card
D SIM Card
K SIM card UICC
F  ~
$ENDCMP
#
$CMP SIM_Card_Shielded
D SIM Card
K SIM card UICC
F  ~
$ENDCMP
#
$CMP SODIMM-200
D SODIMM 200 Pin socket
K SODIMM SO-DIMM DDR1 DDR2
F ~
$ENDCMP
#
$CMP SODIMM-200_Split
D SODIMM 200 Pin socket
K SODIMM SO-DIMM DDR1 DDR2
F ~
$ENDCMP
#
$CMP Samtec_ASP-134602-01
D Connector array, 10x40, 1.27mm pitch, male pins, gold finish, VITA 57.1 FMC, SMD
K FPGA Mezzanine Card FMC Terminal Connector Header
F http://suddendocs.samtec.com/prints/asp-134602-01-mkt.pdf
$ENDCMP
#
$CMP Screw_Terminal_01x01
D Generic screw terminal, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x02
D Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x03
D Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x04
D Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x05
D Generic screw terminal, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x06
D Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x07
D Generic screw terminal, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x08
D Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x09
D Generic screw terminal, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x10
D Generic screw terminal, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x11
D Generic screw terminal, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x12
D Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x13
D Generic screw terminal, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x14
D Generic screw terminal, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x15
D Generic screw terminal, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x16
D Generic screw terminal, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x17
D Generic screw terminal, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x18
D Generic screw terminal, single row, 01x18, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x19
D Generic screw terminal, single row, 01x19, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x20
D Generic screw terminal, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP SpeakON_NL2
D speakON Connector, Male or Female, NL2
K speakon connector
F http://www.neutrik.com/en/speakon/
$ENDCMP
#
$CMP SpeakON_NL4
D speakON Connector, Male or Female, NL4
K speakon connector
F http://www.neutrik.com/en/speakon/
$ENDCMP
#
$CMP SpeakON_NL4_Switch
D speakON Connector, Male or Female, NL4, Switched Pins
K speakon connector
F http://www.neutrik.com/en/speakon/
$ENDCMP
#
$CMP SpeakON_NL8
D speakON Connector, Male or Female, NL8
K speakon connector
F http://www.neutrik.com/en/speakon/
$ENDCMP
#
$CMP TestPoint
D test point
K test point tp
F ~
$ENDCMP
#
$CMP TestPoint_2Pole
D 2-polar test point
K point tp
F ~
$ENDCMP
#
$CMP TestPoint_Alt
D test point (alternative shape)
K test point tp
F ~
$ENDCMP
#
$CMP TestPoint_Flag
D test point (alternative flag-style design)
K test point tp
F ~
$ENDCMP
#
$CMP TestPoint_Probe
D test point (alternative probe-style design)
K test point tp
F ~
$ENDCMP
#
$CMP TestPoint_Small
D test point
K test point tp
F ~
$ENDCMP
#
$CMP UEXT_Host
D Universal EXTension (UEXT) is a connector layout which includes power and three serial buses: Asynchronous, I2C, and SPI
K UEXT, SPI, UART, I2C
F https://www.olimex.com/Products/Modules/UEXT/resources/UEXT_rev_B.pdf
$ENDCMP
#
$CMP UEXT_Slave
D Universal EXTension (UEXT) is a connector layout which includes power and three serial buses: Asynchronous, I2C, and SPI
K UEXT, SPI, UART, I2C
F https://www.olimex.com/Products/Modules/UEXT/resources/UEXT_rev_B.pdf
$ENDCMP
#
$CMP USB3_A
D USB 3.0 A connector
K usb universal serial bus
F ~
$ENDCMP
#
$CMP USB3_B
D USB 3.0 B connector
K usb universal serial bus
F ~
$ENDCMP
#
$CMP USB_A
D USB Type A connector
K connector USB
F  ~
$ENDCMP
#
$CMP USB_B
D USB Type B connector
K connector USB
F  ~
$ENDCMP
#
$CMP USB_B_Micro
D USB Micro Type B connector
K connector USB micro
F ~
$ENDCMP
#
$CMP USB_B_Mini
D USB Mini Type B connector
K connector USB mini
F ~
$ENDCMP
#
$CMP USB_C_Plug
D USB Type-C Plug connector
K usb universal serial bus
F https://www.usb.org/sites/default/files/documents/usb_type-c.zip
$ENDCMP
#
$CMP USB_C_Plug_USB2.0
D USB 2.0-only Type-C Plug connector
K usb universal serial bus type-C USB2.0
F https://www.usb.org/sites/default/files/documents/usb_type-c.zip
$ENDCMP
#
$CMP USB_C_Receptacle
D USB Full-Featured Type-C Receptacle connector
K usb universal serial bus type-C full-featured
F https://www.usb.org/sites/default/files/documents/usb_type-c.zip
$ENDCMP
#
$CMP USB_C_Receptacle_USB2.0
D USB 2.0-only Type-C Receptacle connector
K usb universal serial bus type-C USB2.0
F https://www.usb.org/sites/default/files/documents/usb_type-c.zip
$ENDCMP
#
$CMP USB_OTG
D USB mini/micro connector
K connector USB
F  ~
$ENDCMP
#
$CMP Wuerth_7499010121A
D LAN Transformer Jack, RJ45, 10/100 BaseT
K lan jack transformer
F http://katalog.we-online.de/pbs/datasheet/7499010121A.pdf
$ENDCMP
#
$CMP Wuerth_7499151120
D Dual LAN Transformer Jack, RJ45, 10/100/1000 BaseT
K dual lan jack transformer
F http://katalog.we-online.de/pbs/datasheet/7499151120.pdf
$ENDCMP
#
$CMP XLR3
D XLR Connector, Male or Female, 3 Pins
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack2_Combo
D XLR (Male or Female) and Audio Jack (Mono / TS) Combo Connector, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack2_Combo_Ground
D XLR (Male or Female) and Audio Jack (Mono / TS) Combo Connector, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack3_Combo
D XLR (Male or Female) and Audio Jack (Stereo / TRS) Combo Connector, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack3_Combo_Ground
D XLR (Male or Female) and Audio Jack (Stereo / TRS) Combo Connector, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack3_Combo_GroundSwitch_Switch
D XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector, Discrete Switched Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack3_Combo_Ground_Switch
D XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_AudioJack3_Combo_Switch
D XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_Ground
D XLR Connector, Male or Female, 3 Pins, Discrete Ground Pin
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_Ground_Switched
D XLR Connector, Male or Female, 3 Pins, Discrete Ground Pin, SPDT Switch
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR3_Switched
D XLR Connector, Male or Female, 3 Pins, SPDT Switch
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR4
D XLR Connector, Male or Female, 4 Pins
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR5
D XLR Connector, Male or Female, 5 Pins
K xlr connector
F  ~
$ENDCMP
#
$CMP XLR6
D XLR Connector, Male or Female, 6 Pins
K xlr connector
F  ~
$ENDCMP
#
#End Doc Library
