(footprint "nice_view_1side" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5F8C836B)
  (descr "Connecteur 6 pins")
  (tags "CONN DEV")
  (attr through_hole)
  (fp_text reference "J2" (at 3.7 2.1 180) (layer "F.Fab")
    (effects (font (size 0.8128 0.8128) (thickness 0.15)))
    (tstamp 56f2280e-a38f-400f-8c55-81ec4ba13b5b)
  )
  (fp_text value "OLED" (at 3.6 3.3) (layer "F.SilkS") hide
    (effects (font (size 0.8128 0.8128) (thickness 0.15)))
    (tstamp dbe0e00e-ee13-4ff5-9ed6-9e730d15a0fd)
  )
  (fp_text user "nice!view" (at 5.07 -2.1) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 546a7e9a-9866-4d99-965e-9a201be0662f)
  )
  (fp_line (start -1.15 -1.15) (end 11.29 -1.15) (layer "F.SilkS") (width 0.15) (tstamp 3a32a334-0179-4e81-ab53-2b936f5ba6b0))
  (fp_line (start -1.15 1.15) (end 11.29 1.15) (layer "F.SilkS") (width 0.15) (tstamp a51e66d5-1d52-443c-9336-c601a7f7238e))
  (fp_line (start -1.15 1.15) (end -1.15 -1.15) (layer "F.SilkS") (width 0.15) (tstamp adbe6ee1-e426-4624-96ba-b45a4a620af0))
  (fp_line (start 11.29 -1.15) (end 11.29 1.15) (layer "F.SilkS") (width 0.15) (tstamp d01984f2-1c30-4d20-a7b8-30d4cba1c0ee))
  (pad "1" thru_hole oval (at 0 0) (size 1.397 1.778) (drill 0.8128) (layers *.Cu "B.Mask") (tstamp 4291a49e-edf6-49c4-b6b3-9a2a9a1b45c3))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.397 1.778) (drill 0.8128) (layers *.Cu "B.Mask") (tstamp 79c47f26-d9b9-4bdb-88e5-0023d0721463))
  (pad "3" thru_hole oval (at 5.08 0) (size 1.397 1.778) (drill 0.8128) (layers *.Cu "B.Mask") (tstamp c68df3a8-5eab-49ec-b728-854292682696))
  (pad "4" thru_hole oval (at 7.62 0) (size 1.397 1.778) (drill 0.8128) (layers *.Cu "B.Mask") (tstamp fc95fabb-535a-48ae-9a0a-c37fd8f7d81b))
  (pad "5" thru_hole oval (at 10.16 0) (size 1.397 1.778) (drill 0.8128) (layers *.Cu "B.Mask") (tstamp 739f32c0-4ecf-4974-bdeb-a2a6a4cf89f9))
  (model "/Users/foostan/src/github.com/foostan/kbd/kicad-packages3D/kbd.3dshapes/pin-header-1x4.step"
    (offset (xyz 3.8 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "/Users/foostan/src/github.com/foostan/kbd/kicad-packages3D/kbd.3dshapes/OLED-Module-with-Pins.step"
    (offset (xyz 3.8 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
